Standard Operating Procedure

**Tetramethylsilane**

*This is an SOP template and is not complete until: 1) lab specific information is entered into the box below 2) lab specific protocol/procedure is added to the protocol/procedure section and
3) SOP has been signed and dated by the PI and relevant lab personnel.*

 Print a copy and insert into your
*Laboratory Safety Manual* and *Chemical Hygiene Plan*.
Refer to instructions for assistance.

|  |  |
| --- | --- |
| **Department:** | Click here to enter text. |
| **Date SOP was written:** | Click here to enter a date. |
| **Date SOP was approved by PI/lab supervisor:** | Click here to enter a date. |
| **Principal Investigator:** | Click here to enter text. |
| **Internal Lab Safety Coordinator/Lab Manager:** | Click here to enter text. |
| **Lab Phone:** | Click here to enter text. |
| **Office Phone:** | Click here to enter text. |
| **Emergency Contact:** | Click here to enter text. |
| *(Name and Phone Number)* |
| **Location(s) covered by this SOP:** | Click here to enter text. |
| *(Building/Room Number)* |

**Type of SOP:** [ ]  Process [x] Hazardous Chemical [ ]  Hazardous Class

**Purpose**

Tetramethylsilane (TMS) is an extremely **flammable**, **pyrophoric** chemical that has the ability to spontaneously ignite in contact with air. TMS is a building block in organometallic chemistry but also finds use in diverse niche applications. In chemical vapor deposition, TMS is the precursor to silicon dioxide or silicon carbide, depending on the deposition conditions. TMS is the accepted internal standard for calibrating chemical shift for 1H, 13C and 29Si NMR spectroscopy in organic solvents (where TMS is soluble). Because of its high volatility, TMS can easily be evaporated, which is convenient for recovery of samples analyzed by NMR spectroscopy.

**Physical & Chemical Properties/Definition of Chemical Group**

CAS#: 75-76-3

Class: **Pyrophoric and Extremely Flammable**

Molecular Formula: C4H12Si

Form (physical state): Liquid

Color: Colorless

Boiling point: 26-28OC

**Potential Hazards/Toxicity**

Vapors may form explosive mixture or spontaneously ignite with contact in air. May be harmful through inhalation, ingestion, and skin contact. Causes eye, skin, and respiratory tract irritation.

**Personal Protective Equipment (PPE)**

**Respiratory Protection**

Tetramethylsilane should always be used with engineering controls in place. If a respirator is the sole means of protection, please use a full-face supplied air respirator.

Respirators should be used only under any of the following circumstances:

* As a last line of defense (i.e., after engineering and administrative controls have been exhausted).
* When Permissible Exposure Limit (PEL) has exceeded or when there is a possibility that PEL will be exceeded.
* Regulations require the use of a respirator.
* An employer requires the use of a respirator.
* There is potential for harmful exposure due to an atmospheric contaminant (in the absence of PEL).
* As PPE in the event of a chemical spill clean-up process.

Lab personnel intending to use/wear a respirator mask must be trained and fit-tested by ORS and should contact occhealt@uga.edu. This is a UGA requirement described in more detail in the [UGA Respiratory Protection Plan](https://esd.uga.edu/sites/default/files/respiratoryprotection.pdf) and supported by the [Office of Research Occupational Health and Safety Program](https://research.uga.edu/ohsp/).

**Hand Protection**

Please use the glove box gloves and sleeves or if this chemical is handled in a closed system in a certified fume hood, nitrile gloves are recommended.

NOTE: Consult with your preferred glove manufacturer to ensure that the gloves you plan on using are compatible with tetramethylsilane.

Refer to glove selection chart from the links below:

<http://www.ansellpro.com/download/Ansell_8thEditionChemicalResistanceGuide.pdf>

OR

<http://www.allsafetyproducts.biz/page/74172>

OR

<http://www.showabestglove.com/site/default.aspx>

OR

<http://www.mapaglove.com/>

**Eye Protection**

Wear ANSI-approved safety glasses or chemical splash goggles and a face shield.

**Skin and Body Protection**

Wear full-length pants or its equivalence, closed toe shoes, and a flame-resistant lab coat.

**Hygiene Measures**

Handle in accordance with good industrial hygiene and safety practice. Wash hands before breaks and at the end of workday.

**Engineering Controls**

Tetramethylsilane should be used in a glove box filled with inert gas, or in a closed system in a certified fume hood.

**First Aid Procedures**

**If inhaled**

If breathed in, move person into fresh air. If not breathing, give artificial respiration. Consult a physician.

**In case of skin contact**

Wash off with soap and plenty of water for at least 15 minutes. Consult a physician.

**In case of eye contact**

Flush eyes with water as a precaution for at least 15 minutes.

**If swallowed**

Do NOT induce vomiting. Never give anything by mouth to an unconscious person. Rinse mouth with water. Consult a physician.

**Special Handling and Storage Requirements**

**Precautions for safe handling**

Avoid inhalation of vapor or mist. Use explosion-proof equipment. Keep away from sources of ignition - No smoking. Take measures to prevent the build-up of electrostatic charge.

**Conditions for safe storage**

Store in cool place. Keep container tightly closed in a dry and well-ventilated place. Containers which are opened must be carefully resealed and kept upright to prevent leakage. Recommended storage temperature: 2 - 8 °C. Over time, pressure may increase causing containers to burst Handle and open container with care. Avoid storing next to strong acids, strong bases, and strong oxidizers.

**Spill and Accident Procedure**

**Chemical Spill Dial 911**

**24-7 On-Call Response to Research, Environment, Health or Safety Concerns Dial 2-5561 from a campus phone or 706-542-5561 from a non-campus line.**

**Spill** – Follow the procedures set out in the [UGA Chemical and Laboratory Safety Manual.](http://research.uga.edu/docs/units/safety/manuals/Chemical-Laboratory-Safety-Manual.pdf)

[If there are any chemical-specific protocols for responding to a spill, insert them here or mark “none”:]

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# **Medical Emergency Dial 911**

**Life Threatening Emergency, After Hours, Weekends and Holidays** – Dial **911** or the emergency phone numbers listed at the beginning of the UGA Chemical and Laboratory Safety Manual.

*Note: All incidents that result in an injury or property damage must be reported to ORS / ESD using a University Incident/Accident Report.*

**Non-Life-Threatening Emergency** – Follow the instructions in the UGA Chemical and Laboratory Safety Manual.

*Note: All incidents that result in an injury or property damage must be reported to ORS / ESD using a University Incident/Accident Report.*

**Decontamination/Waste Disposal Procedure**

**For general hazardous waste disposal procedures, see Appendix H of the UGA Chemical and Laboratory Safety Manual.**

**Chemical Specific Procedures: [to be inserted or marked as “none”]**

**Safety Data Sheet (SDS) Location**

UGA personnel can access Online SDS through a link in the upper left corner of the ESD home page (<https://esd.uga.edu>) and logging in by using their UGA email user name and password.

**Protocol/Procedure (Add lab specific Protocol/Procedure here)**

Click here to enter text.

**NOTE**

Any deviation from this SOP requires approval from PI.

**Documentation of Training** (signature of all users is required)

* Prior to conducting any work with tetramethylsilane, designated personnel must provide training to his/her laboratory personnel specific to the hazards involved in working with this substance, work area decontamination, and emergency procedures.
* The Principal Investigator must provide his/her laboratory personnel with a copy of this SOP and access to the SDS provided by the manufacturer.
* The Principal Investigator must ensure that his/her laboratory personnel have attended appropriate laboratory safety training or refresher training within the last 12 months.

**Principal Investigator SOP Approval**

Print name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Signature\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Approval Date:

I have read and understand the content of this SOP:

|  |  |  |
| --- | --- | --- |
| **Name** | **Signature** | **Date** |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |
| Click here to enter text. |  | Click here to enter a date. |